%% 3.Frequency response of Second order systems

clc;

clear;

s = tf('s');

G = 25/(s^2 + 5\*s + 25);

figure(1);

step(G)

figure(2)

bode(G)