%%Frequency Response of Second Order System

n=[356]

d=[1 22 356]

G=tf(n,d)

figure(1)

bode(G)

